**\*Lähettäjän tulee aina täyttää kaikki lomakkeeseen sinisellä merkityt tiedot.
\*Vihreällä merkityt tiedot lähettäjän tulee täyttää, mikäli lähetys lastataan lähettäjän toimesta suoraan ulkomaan yksikköön.**

**MULTIMODAL DANGEROUS GOODS FORM**This form may be used as a dangerous goods declaration as it meets the requirements of SOLAS 74, chapter VII, regulation 4; MARPOL 73/78, Annex III, regulation 4

|  |  |
| --- | --- |
| 1  Shipper/Consignor/Sender **\*Lähettäjän nimi ja osoite** | 2  Transport document number |
| 3  Page 1 of      pages | 4  Shipper's reference |
|   | 5  Freight Forwarder's reference |
| 6  Consignee | 7  Carrier (to be completed by the carrier) |
| **\*Vastaanottajan nimi ja osoite** | **SHIPPER'S DECLARATION**I hereby declare that the contents of this consignment are fully and accurately described below by the Proper Shipping Name, and are classified, packaged, marked and labelled/placarded and are in all respects in proper condition for transport according to the applicable international and national governmental regulations. |
| 8  This shipment is within the limitations prescribed for:   (Delete non-applicable) | 9  Additional handling information **TÄYTTÖMALLI**  |
| PASSENGER AND CARGOAIRCRAFT | CARGO AIRCRAFTONLY |
| 10  Vessel/flight no. and date   | 11  Port/place of loading   |
| 12  Port/place of discharge   | 13  Destination   |
| 14  Shipping marks           [\*](file:///C%3A%5CDocuments%20and%20Settings%5Cmspinard%5CLocal%20Settings%5CTemp%5C54.htm#null#null)Number and kind of packages; description of goods          Gross mass (kg)      Net mass (kg)       Cube (m3) |
| **\*Vaarallisen aineen/aineiden tiedot:** **(Katso vaadittavat tiedot lomakkeen alareunasta tähdellä merkitystä kohdasta DANGEROUS GOODS.)**    |
| 15  Container identification No./ vehicle registration No.  | 16  Seal number(s)  | 17  Container/vehicle size & type  | 18  Tare mass (kg)  | 19  Total gross mass (including tare) (kg)  |
| **CONTAINER/VEHICLE PACKING CERTIFICATE**I hereby declare that the goods described above have been packed/ loaded into the container/vehicle identified above in accordance with the applicable provisions. [†](file:///C%3A%5CDocuments%20and%20Settings%5Cmspinard%5CLocal%20Settings%5CTemp%5C54.htm#null#null)**MUST BE COMPLETED AND SIGNED FOR ALL CONTAINER/VEHICLE LOADS BY PERSON RESPONSIBLE FOR PACKING/LOADING.** | 21  RECEIVING ORGANISATION RECEIPT Received the above number of packages/containers/trailers in apparent good order and condition unless stated hereon: RECEIVING ORGANISATION REMARKS: |
|
|
| 20  Name of company:**\*Lastauksen suorittavan yrityksen nimi** | Haulier's nameVehicle reg. no.Signature and date | 1. Name of company (OF SHIPPER PREPARING THIS NOTE)

**\*Lähettävän yrityksen nimi**  |
| Name/Status of declarant**\*Vastuuhenkilön nimi ja asema** | Name/status of declarant**\*Vastuuhenkilön nimi ja asema** |
| Place and date**\*Paikka ja päivämäärä** | Place and date**\*Paikka ja päivämäärä** |
| Signature of declarant**\*Vastuuhenkilön allekirjoitus**  | DRIVER'S SIGNATURE  | Signature of declarant**\*Vastuuhenkilön allekirjoitus** |

**\* DANGEROUS GOODS:**
You must specify: UN No., Proper Shipping Name, hazard class, packing group, (where assigned) marine pollutant and observe the mandatory requirements under applicable national and international governmental regulations. For the purposes of the IMDG Code see [5.4.1.4](file:///C%3A%5CDocuments%20and%20Settings%5Cmspinard%5CLocal%20Settings%5CTemp%5C54.htm#5.4.1.4#5.4.1.4)

† For the purposes of the IMDG Code, see [5.4.2](file:///C%3A%5CDocuments%20and%20Settings%5Cmspinard%5CLocal%20Settings%5CTemp%5C54.htm#5.4.2#5.4.2)

**Documentary Aspects of the International Transport of Dangerous Goods**

**Container/Vehicle Packing Certificate**

|  |  |
| --- | --- |
| The signature given overleaf in Box 20 must be that of the person controlling the container/vehicle operation.It is certified that:The container/vehicle was clean, dry and apparently fit to receive the goods.If the consignments include goods of class 1, other than division 1.4, the container is structurally serviceable.No incompatible goods have been packed into the container/vehicle unless specially authorised by the Competent Authority.All packages have been externally inspected for damage and only sound packages packed.Drums have been stowed in an upright position, unless otherwise authorised by the Competent Authority.All packages have been properly packed and secured in the container/vehicle. | When materials are transported in bulk packagings the cargo has been evenly distributed in the container/vehicle.The packages and the container/vehicle have been properly marked, labelled and placarded. Any irrelevant mark, labels and placards have been removed.When solid carbon dioxide (CO2 - dry ice) is used for cooling purposes, the vehicle or freight container is externally marked or labelled in a conspicuous place, e.g. at the door end, with the words: DANGEROUS CO2 GAS (DRY ICE) INSIDE - VENTILATE THOROUGHLY BEFORE ENTERING.When this Dangerous Goods Form is used as a container/vehicle packing certificate only, not a combined document, a dangerous goods declaration signed by the shipper or supplier must have been issued/received to cover each dangerous goods consignment packed in the container.**Note:** The container packing certificate is not required for tanks |

|  |  |
| --- | --- |
| 1  Shipper/Consignor/Sender | 2  Transport document number |
| 3  Page      of      pages | 4  Shipper's reference |
|   | 5  Freight Forwarder's reference |
| 14  Shipping marks           \*Number and kind of packages; description of goods          Gross mass (kg)      Net mass (kg)      Cube (m3) |
|                           |